# DISCONTINUED PRODUCT

## Only spare parts available.

Gamespot - Spot Score - Very Good. "... guaranteed to bring you deeper into the game than ever before... extreme gaming toy is sure to amaze even the most jaded gamer with the new intensity it brings to the gaming experience. Digital Gamer - 4.5 stars

Displays
| Individual lens focus and IPD adjustments
| 3D stereoscopic Smart Visor - 789(RGB)x230 resolution x 2 263x230 True Pixels
| Dual 0.7" colour liquid crystal displays (181,470 pixels)
| 256 Colours
| Picture size: vertical = 10.6 mm horizontal = 14.3 mm Provides an image of a 35 ft.screen at a distance of 35 feet
Optics
| Field of view (FOV) vertical = 26.4 degrees horizontal = 35.5 degrees diagonal = 45.0 degrees
Virtual Orientation System (VOS) Head Tracker
| Angular range: vertical = +/- 70 degrees horizontal = 360 degrees
| Angular resolution: vertical = 0.077 degrees horizontal = 0.251 degrees
| Three degrees of freedom: yaw (azimuth):360 degrees pitch (elevation):+/- 70 degrees roll (tilt):+/- 70 degrees
VFX1 Interface Protocol (VIP) Card
| Interfaces with standard VGA feature connector 26-pin ribbon cable
| 60Hz Refresh Rate (60 times per second) - up to 1 kHz refresh rate possible
| Utilises ACCESS.bus Connectivity Standard Accepts 125 simultaneous devices 100 Kbit/sec transfer rate
| Does NOT require serial port connection
Connections
| Single 26-pin D-connector (High resolution) containing video, audio and VOS head tracking sensor cable
| Connects to VFX1 Interface Protocol (VIP) card
| ACCESS.bus host connector (Phone Jack Connector)
| VIP interfaces with standard VGA feature connector
| 2 cables from stereo sound card to VIP card (for headphones and microphone)
| VIP card requires 8 bit PC ISA slot
Video
| Dual active matrix colour LCDs
| Works with existing Standard VGA applications
Audio
| High fidelity stereo headphones designed by AKG of Austria: 20 Hz - 20 kHz
| Interfaces with any standard PC stereo sound card's amp/line out connector
| For 3D sound, use a 3D capable sound card eg: GUS ACE or Sonic Storm
Comset Microphone
| Hands free communication
| Gamer to gamer
| Voice recognition capable
Adjustments
| Smart Visor rotates up and out of the way when not immersed in VR world
| Smart Visor rotates down and adjusts for closeness to the face
| Removal of the headset is not necessary when interfacing outside the headset
| Fully adjustable InterPupillary Distance (IPD)
| Individual eye focus adjustment (for use with and without glasses)
| Rear adjustable strap for comfortable fit
Power Requirements
| 5 volts, 2 watts
| 0.4 amps (with Cyberpuck Connected)
One Year Warranty
| The VFX1 Headgear VR System has a One Year warranty against defects in materials or workmanship

| IBM PC or compatible 386, 486, Pentium +
| Video card (VGA minimum) with 100% VESA standard compliant feature connector (ISA, VLB, PCI)
| Free ISA Expansion Slot
| One free base port: 260, 280, 2A0, 2C0
| One free IRQ: 5, 7, 10, 11, 12, 15
| Stereo-capable soundcard (for audio)

    Copyright © 2003 Mindflux (Jasandre Pty. Ltd.). All rights reserved.
    info@mindflux.com.au   Ph: (02) 9416 9619   Fax: (02) 9416 9029