| ## VFX1 Technical Specifications |
3D Stereoscopic Flip-Up Visor · With focus and IPD adjustments · High contrast color video · Dual 0.7 color liquid crystal displays · 181,740 pixels per LCD · Works with existing, standard VGA applications · 120" screen at 11 feet Optics · Field of view - vertical - 26.4 degrees horizontal degrees diagonal - 45.0 degree · High quality color corrected optics · Provides large screen stereoscopic (3D video) imaging Virtual Orientation System (VOS™) Sourceless Head Tracker · With three degrees of freedom · Yaw (azimuth): 360 degrees · Pitch (elevation): +/- 70 degrees · Roll (tilt): +/- 70 degrees VFX1 HEADGEAR Interface Protocol (VIP™) Card · Interfaces with standard VGA card and sound card · Includes ACCESS.bus host · Connect up to 125 different devices · Does not require serial port connection Cyberpuck™ VR Controller · Left or right-handed control · ACCESS.bus device · 3 programmable buttons · Lightweight (3 oz.) · Free floating design High Quality Stereo Headphones · Designed by AKG of Austria · 20 Hz - 20 kHz · Stereo and 3D sound capable Comset™ Microphone · Hands free communications · Multiplayer communications · Voice recognition capable Ergonomic Design · Comfort · Control · Extended use Power Requirements · 5 volts, 2.0 watts · 0.4 amps (with Cyberpuck controller) · Does not require external power sources System Requirements · IBM PC or compatible, 386, 486, Pentium or better · VGA card (ISA, VLB, PCI) with VESA Standard Feature Connector · Free expansion slot · Stereo sound card (for audio) Manufacturers Suggested Retail Price · $695 w/Vip Card and Cyberpuck This information is subject to change without notice copyright 1998-99