| ## VFX3D vs. VFX1 |
Description | VFX3D | VFX1
Display Resolution | Dual 0.7 inch colorLCD's 360,000 Pixels per LCD 1600x1200 maximum resolution Stereo Video 2X better than the original VFX1. | Dual 0.7 inch color LCD's 180,000 Pixels per LCD 640x480 maximum resolution Stereo Video
Optics | Fixed Focus No IPD adjustment Eyeglass friendly Brightness, Color,Contrast controlls 100% Improvement | Focusing IPD Adjustable Difficult eyeglass use
Tracking | Solid State Silicon Based Accelerometer 100% Improvement | Fluxgate
PC Interface | VGA/232 Supports all video cards Supports 3D acceleration Full 3D stereo video with many DirectX titles S-video support 100% Improvement | VIP Card (internal installation required) 256 color depth required
Software | VFX Control Panel - OSD control switch - Stereo video control VFXLauncher Brightness, color,contrast and Volume control Single Launcher for all titles | Patche configuration required for most titles No control over video settings